Special Station_Id's:
NEXRAD
A2M
HRR
COMPUTE
COMPUTE-Get
COMPUTE-Put
ROUTE
SHELL
SNOWMELT
FORECAST
AFWS
LOOKUP
FILE
RUN
MRUN
IF
SET-INTERVAL
KISTERS

Datatype_Id's  1 to 32.
Site_Id's  0 to 999.  
Datatype_Site_Id's= Datatype_Id & Site_Id (ex: elev 3 site 1= 3001)

Datatype_Site_Id's -32,768 to 32,767 minimum 4 characters.  Tip: Use
negative DSID's for computed values.


               Table of datatype_id’s
datatype_id  datatype_name  unit_name  rounding  averaging
1 flow	 cfs	 usgs	 avg
2 gage height	 ft	 0.00	 avg
3 elevation	 ft	 0.00	 avg
4 contents	 kaf	 usgs	 ending
5 contents	 % capacity	 0.0	 avg
6 specific conductance	 umhos	 usgs	 avg
7 water temperature	 °f	 0.0	 avg
8 ph	 std units	 usgs	 avg
9 total precip	 inches	 0.00	 ending
10 rainfall	 inches	 0.00	 increment	see below
11 adj radar/snowmelt	 inches	 0.00	 increment	see below
12 turbidity	 fnu	 usgs	 avg
13 dissolved oxygen	 % saturation	 usgs	 avg
14 tds	 mg/l	 usgs	 avg
15 pressure	 in hg	 0.00	 avg
16 dew point	 °f	 0.0	 avg
17 air temperature	 °f	 0.0	 avg
18 humidity	 % saturation	 usgs	 avg
19 wind direction	 0.25	 weighted
20 wind gust	 mph	 usgs	 avg
21 snow depth	 inches	 0.0	 avg
22 absolute humidity	 g/m3	 usgs	 avg
23 snow water content	 inches	 0.00	 ending
24 inflow	 cfs	 usgs	 avg
25  	  	 NONE	 avg
26 		 % of	 avg	 0.0	 avg
27 ET	 inches	 0.00	 increment
28 wind speed	 mph	 usgs	 avg
29 solar radiation	 Langley’s/day	 usgs	 avg
30 runoff	 cfs	 usgs	 avg
31   		 NONE	 avg
32 nexrad maximum	 what ever	 usgs	 avg

For datatypes not listed, except for reserved datatypes, you can rename 
any of the other datatypes that match your rounding and averging needs.

Important:  Datatype_name 'ratio' is reserved for rainfall adjustment and usually associated with datatype_id=31, but all other names can be changed.

Datatype_id's with special associated computations:  19=wind direction,
27=ET, 29=solar & long radiation, 30=runoff, 32=radar image maximum.

For runoff datatype_id 30 computations, daily datatype_id's 4, -4, and 5 end of day condtions will be written secretly so be aware.
Runoff datatype_ID's for end of day in rday:
datatype_ID 3 = Runoff Excess as inch/hr (if 'Write unit CN P, S').
datatype_ID 4 = Soil Storage or Initial Loss (always end of day).
datatype_ID -4 = Pricip residual (always end of day).
datatype_ID 5 = Groundwater flow (always end of day).

Useful dsid's in table rupdate:
datatype_ID 0 has site_name as last error.
datatype_ID -1 has value as next scheduled run date.


Rainfall datatype_ID compatibility conventions:
 10xxx rain gage
-10xxx radar rainfall
-11xxx adjusted radar
 11xxx, -23xxx snowmelt and swc

Datatype_id's 10 & 11 rainfall, 23 SWC, and 27 ET unit values rounded as 0.00000 and hourly's 0.0000.

USGS rounding means:
 0
 0.001 - 0.099
 0.01 - 0.99
 1.0 - 9.9
 10.0 - 99.9
 100 - 999 
 1010 - 9999990


'SOURCE' codes for the data sources used the the values tables: 
0=Canada Wateroffice
1=Wunderground
2=USGS
3=CalDEC
4=USCS Snotel
5=WRITE PROTECT
6=USBR
7=COE
8=CIMIS
9=RADAR
10=ROUTE
11=COMPUTE
12=SNOWMELT
13=FILE  (yes 13 was a screw up)
13=Real radar rainfall values from GETNEXRAD.exe
14=Storm track rainfall Nowcast from GETNEXRAD.exe or Wizard edit
15=NWS QPF rainfall forecasts from GETNEXRAD.exe
16=SHELL (example Hec-Ras routing)
17=COMPUTE-Get
18=FORECAST-NWS  (6 hour QPF, 6 hour flow/stage)
19=AFWS
20=Lookup
21=KISTERS
22=HCFCD
23=MRMS-A2M radar rain rate
24=MRMS-HRR Forecast
25=Spotwx's Forecast-RAP, HRRR, NAM, SREF, GFS, HRDPS, RDPS, GDPS, GEPS


Stadard Meridians, Std Time Offset, DST Offset
Atlantic -60º -4 -3
Eastern -75º -5 -4
Central -90º -6 -5
Mountain -105º -7 -6
Pacific -120º -8 -7
Alaska -135º -9 -8
Hawaii-Aleutian -150º -10 -9


SETUP PATHS THAT NEED RESET FOR NEW INSTALLS OR COPING OF SETUPS:

In GetRealtime foler file GetRealtime_setup.txt:

  GetAccess.exe folder=C:\GETPROJECTS\GETONEIDACR2\GETACCESS\
  GetGraphs.exe folder=C:\GETPROJECTS\GETONEIDACR2\GETGRAPHS\
  GetNexrad.exe folder=C:\GETPROJECTS\GETONEIDACR2\GETNEXRAD\
  NowCast Info folder=C:\GETPROJECTS\GETONEIDACR2\GETNEXRAD\
  Gage Avg OnOff folder=C:\GETPROJECTS\GETONEIDACR2\GETGRAPHS\
and
  Database Connection String=Provider=Microsoft.Jet.OLEDB.4.0;Data Source=C:\GetProjects\GetOneidaCr2\GetAccess\GetAccessHDB_BGM2.mdb;User Id=admin;Password=;

In GetAcess folder:  

  GetAccess_setup.txt

In GetGraphs folder:

  GetGraphs_setup.txt
  and a copy of GetAccess_setup.txt for GetFromAccessNow.exe

In GetNexrad folder:

  GetNexradHDB.txt

I think thats all the paths.