Future Days=5
Percent Missing Allowed= 100%
Write Dailys= True
Write Hourly Avg= True
Write Daily Max= True
Write Unit Values= True
Write Unit Shifts= False
Overwrite Protected Source 5= True
Check for Possible Bad Values= False
Possible Bad Value Change= 200%
Last Runoff Run's Storage= True
Minutes between retrievals=30
Max hours of radar=2
Save Radar greater than= False
Beep on Save= True
Delete temporary internet files=True
Loop radar boundaries=True
Use Nexrad Ridge1 full web file listing=False
Use Nexrad short web file listing=False
Use Nexrad Ridge2 Iowa State Mesonet=True
Compact and Backup HDB at midnight= True
GetAccess.exe folder=C:\GETONEIDACR\GETACCESS\
GetGraphs.exe folder=C:\GETONEIDACR\GETGRAPHS\
GetNexrad.exe folder=C:\GETONEIDACR\GETNEXRAD\
NowCast Info folder=C:\GETONEIDACR\GETNEXRAD\
Gage Avg OnOff folder=C:\GETONEIDACR\GETGRAPHS\
Radar Boundary File folder=
Menu Pic=C:\GETONEIDACR\GETREALTIME\ONEIDAAREA.JPG
Menu Text Color= 0 
Minimize to System Tray=True
Column Widths=1380,1155,840,4050,780,2265,5025
Alert Address=
Alert Address CC=
Alert Address BCC=
Don't Ask Questions=False
Create Winds Aloft graphic file=True
Metric Units=False

Database Connection String=Provider=Microsoft.Jet.OLEDB.4.0;Data Source=C:\GetOneidaCr\GetAccess\GetAccessHDB_BGM.mdb;User Id=admin;Password=;

Station_ID; Datatype_Site_ID; Datatype_Name; Site_Name; base1; shift1; formula1; base2; shift2; formula2; base3; shift3; formula3
************; ************; ************; *****BGM RADAR*******
Run-NEXRAD-BGM; -10301; Radar Rain; Oneida Cr Sub1, NY; 2; nowcast 3
NEXRAD-BGM; -10302; Radar Rain; Oneida Cr Sub2, NY; 2; nowcast 3
NEXRAD-BGM; -10303; Radar Rain; Oneida Cr Sub3, NY; 2; nowcast 3
NEXRAD-BGM; -10201; Rainfall; ABC Dairy KNYCANAS5, NY; 2
NEXRAD-BGM; -10202; Rainfall; KNYMORRI7 Hilltop Station, NY; 2
NEXRAD-BGM; -10203; Rainfall; White Eagle KNYHAMIL3, NY; 2
NEXRAD-BGM; -10204; Rainfall; KNYCANAS11 Curtin Heifer Barn, NY; 2
NEXRAD-BGM; -10205; Rainfall; Deansboro KNYDEANS2, NY; 2
NEXRAD-BGM; -10206; Rainfall; Lowell KNYROME4, NY; 2
NEXRAD-BGM; -10207; Rainfall; Bartlett KNYWESTM2, NY; 2
NEXRAD-BGM; -10208; Rainfall; KSYR Syracuse Airport, NY; 2
NEXRAD-BGM; -10209; Rainfall; KRME Rome Airport, NY; 2
NEXRAD-BGM; -10210; Rainfall; Teds Farm KNYCAZEN7, NY; 2
NEXRAD-BGM; -10211; Rainfall; Smithfield KNYCANAS10, NY; 2
NEXRAD-BGM; -10212; Rainfall; Erieville KNYERIEV2, NY; 2
************; ************; ************; *****Forecasts*****
Run-FORECAST-NWS; -11301; Forcast Rain; Oneida Cr Sub1, NY; -3; 42.9962,-75.5885,3
FORECAST-NWS; -11302; Forcast Rain; Oneida Cr Sub2, NY; -3; 42.9962,-75.5885,3
FORECAST-NWS; -11303; Forcast Rain; Oneida Cr Sub3, NY, AL; -3; 42.9962,-75.5885,3
FORECAST-NWS; 17200; Temperature; Oneida Cr, NY; -3; 42.9962,-75.5885
FORECAST-NWS; 18200; Humidity; Oneida Cr, NY; -3; 42.9962,-75.5885
FORECAST-NWS; 28200; Windspeed; Oneida Cr, NY; -3; 42.9962,-75.5885
************; ************; ************; *****USGS Gages*****
04243500; 1300; Flow; ONEIDA CR AT ONEIDA, NY
04243500; 2300; Gage Height; ONEIDA CR AT ONEIDA, NY
************; ************; ************; *****Wundergages*******
KNYCANAS5; 17201; Temperature; P1 ABC Dairy, NY
KNYCANAS5; 18201; Humidity; P1 ABC Dairy, NY
KNYCANAS5; 28201; Wind Speed; P1 ABC Dairy, NY
KNYCANAS5; 10201; P1 Rainfall; P1 ABC Dairy, NY
KNYMORRI7; 10202; P2 Rainfall; P2 Hilltop Station, NY
KNYHAMIL3; 17203; Temperature; P3 White Eagle, NY
KNYHAMIL3; 18203; Humidity; P3 White Eagle, NY
KNYHAMIL3; 28203; Wind Speed; P3 White Eagle, NY
KNYHAMIL3; 10203; P3 Rainfall; P3 White Eagle, NY
KNYCANAS11; 10204; P4 Rainfall; P4 Curtin Heifer Barn, NY
KNYCANAS11; 17204; Temperature; Fountain Street, NY
KNYCANAS11; 18204; Humidity; Fountain Street, NY
KNYCANAS11; 28204; Wind Speed; Fountain Street, NY
KNYDEANS2; 17205; Temperature; P5 Deansboro, NY
KNYDEANS2; 18205; Humidity; P5 Deansboro, NY
KNYDEANS2; 28205; Wind Speed; P5 Deansboro, NY
KNYDEANS2; 10205; P5 Rainfall; P5 Deansboro, NY
KNYROME4; 10206; P6 Rainfall; P6 Lowell, NY
KNYWESTM2; 10207; P7 Rainfall; P7 Bartlett, NY
KSYR; 10208; Rainfall; P8 Syracuse Airport, NY
KRME; 10209; Rainfall; P9 Rome Airport, NY
KNYCAZEN7; 10210; P10 Rainfall; P10 Teds Farm, NY
KNYCAZEN7; 17210; Temperature; P10 Teds Farm, NY
KNYCAZEN7; 18210; Humidity; P10 Teds Farm, NY
KNYCAZEN7; 28210; Wind Speed; P10 Teds Farm, NY
KNYCAZEN7; 29210; Solar Radiation; Teds Farm, NY; 0; 0; 2.065*P1
KNYCANAS10; 10211; P11 Rainfall; Smithfield, NY
KNYCANAS10; 17211; Temperature; Smithfield, NY
KNYCANAS10; 18211; Humidity; Smithfield, NY
KNYCANAS10; 28211; Wind Speed; Smithfield, NY
KNYERIEV2; 10212; P12 Rainfall; Erieville, NY
************; ************; ************; *****RATIOS*******
COMPUTE-hour; 10251; Rainfall; Avg Rain Gages Oneida Cr; 0; 0; (P1+P2+P3+P4+P5+P6+P7+P8+P9+P10+P11+P12)/N
COMPUTE-hour; -10251; Rainfall; Avg Rain Radars Oneida Cr; 0; 0; (P1+P2+P3+P4+P5+P6+P7+P8+P9+P10+P11+P12)/N
COMPUTE-hour; -31251; Ratio; Avg G/R Ratio Oneida Cr; 0; .02,1.14, 5; P1/P2
************; ************; ************; *****Adjusted Rainfall*******
COMPUTE-unit; -11301; Adj Rain; Oneida Cr Sub1, NY; 0; -1, 1.14, 0.5, 0.50; P1*P2
Run-COMPUTE-unit; -11302; Adj Rain; Oneida Cr Sub2, NY; 0; -1, 1.14, 0.5, 0.50; P1*P2
COMPUTE-unit; -11303; Adj Rain; Oneida Cr Sub3, NY; 0; -1, 1.14, 0.5, 0.50; P1*P2
COMPUTE-unit; -11201; Adj Rain; Wundergage #1 Adjust; 0; -1, 1.14, 0.5, 0.50; P1*P2
************; ************; ************; *****SNOW CALCS******
COMPUTE-hour; 17200; Avg Temperature; Oneida Cr, NY; -80; 0; (P1+P2+P3)/N+shift
COMPUTE-hour; 18200; Avg Humidity; Oneida Cr, NY; 0; 0; (P1+P2+P3)/N
COMPUTE-hour; 28200; Avg Wind Speed; Oneida Cr, NY; 0; 0; (P1+P2+P3)/N
COMPUTE-unit; 29200; Solar Radiation; Oneida Cr, NY; 0; 42.9962,-75.5885,-120, 630
Run-COMPUTE-unit; -29200; Long Radiation; Oneida Cr, NY; 0
COMPUTE-unit; -27200; ET Grass; Oneida Cr, NY; 0; 42.9962,-75.5885,-120, 630, 0.75
Run-SNOWMELT-unit; 11301,-23301; Melt, SWC; Oneida Cr Sub1, NY; 0; +1, 1, 0.75, 1, 1.01, 1, 1, 34
SNOWMELT-unit; 11302,-23302; Melt, SWC; Oneida Cr Sub2, NY; 0; +0.5, 1, 0.75, 1, 1.005, 1, 1, 34
SNOWMELT-unit; 11303,-23303; Melt, SWC; Oneida Cr Sub3, NY; 0; 0, 1, 0.75, 1, 1, 1, 1, 34
************; ************; ************; *****Runoff******
COMPUTE-unit; -30301; Runoff; Oneida Cr Sub1, NY; 15; 6.0, 86, 0.1, 2, 41.8, 0.5, .17, 0.65, 4, 0.25, 12, 98, 82, 0.85, 0.0, 0.05, 0.3, 0.8, 0.03, 0.8, 0, 0.2, 1, 0.7, 0, Lag0; P1; 0; LittleTallapoosa.DGF
COMPUTE-unit; -30302; Runoff; Oneida Cr Sub2, NY; 15; 7.5, 86, 0.1, 2, 38.4, 0.5, .17, 0.65, 4, 0.25, 12, 98, 82, 0.85, 0.0, 0.05, 0.3, 0.8, 0.03, 0.8, 0, 0.2, 1, 0.7, 0, Lag0; P1; 0; LittleTallapoosa.DGF
COMPUTE-unit; -30303; Runoff; Oneida Cr Sub3, NY; 15; 6.5, 86, 0.1, 2, 34.7, 0.5, .17, 0.5, 4, 0.5, 12, 98, 82, 0.85, 0.0, 0.05, 0.3, 0.8, 0.03, 0.8, 0, 0.2, 1, 0.7, 0, Lag0; P1; 0; LittleTallapoosa.DGF
**IF; -1300; Flow Check; Routed Base Flow For Unit Graph Only; rhour; SKIP-5; P1<80
**COMPUTE-unit; -30301; Runoff; Oneida Cr Sub1, NY; 1; 6.0, 86, 0.1, 2, 41.8, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; VillageCreek.DGF
**COMPUTE-unit; -30302; Runoff; Oneida Cr Sub2, NY; 1; 6.5, 86, 0.1, 2, 38.4, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; VillageCreek.DGF
**COMPUTE-unit; -30303; Runoff; Oneida Cr Sub3, NY; 1; 6.5, 86, 0.1, 2, 34.7, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; VillageCreek.DGF
************; ************; ************; *****Base Flow<80******
**IF; -1300; Flow Check; Routed Base Flow For Unit Graph Only; rhour; SKIP-4; P1>=80
**COMPUTE-unit; -30301; Runoff; Oneida Cr Sub1, NY; 1; 6.0, 86, 0.1, 2, 41.8, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; LittleTallapoosa.DGF
**COMPUTE-unit; -30302; Runoff; Oneida Cr Sub2, NY; 1; 6.5, 86, 0.1, 2, 38.4, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; LittleTallapoosa.DGF
**COMPUTE-unit; -30303; Runoff; Oneida Cr Sub3, NY; 1; 6.5, 86, 0.1, 2, 34.7, 0.5, .17, 0.5, 4, 0.35, 12, 98, 82, 0.85, 0.2, 0.10, 0.3, 0.8, 0.03, 0.8, 0, 0.2, Lag0; P1; 0; LittleTallapoosa.DGF
************; ************; ************; *****Routings*****
Run-ROUTE-unit; -1300; Flow; Route Sub3 And Combine All
LOOKUP-Unit-log-log; -2300; Gage Height>5-daymax; Oneida Cr at Oneida, NY
**COMPUTE-Unit; -2300; Gage Height; Oneida Cr at Oneida, NY; 0; -6; 0.05066*(P1+260+Shift)^0.6591933; 200; -254*(P1-200)/800-6; 0.05066*(P1+260+Shift)^0.6591933; 1000; -260; 0.05066*(P1+260+Shift)^0.6591933
************; ************; ************; *****Daily Curve Numbers*****
COMPUTE-Day; -6301; SCS CN; Oneida Cr Sub1, NY; 0; 0; 1000/(P1+10)
COMPUTE-Day; -6302; SCS CN; Oneida Cr Sub2, NY; 0; 0; 1000/(P1+10)
COMPUTE-Day; -6303; SCS CN; Oneida Cr Sub3, NY; 0; 0; 1000/(P1+10)
END
