Three sub basins on Flamingo Wash Las Vegas Valley <<<some title line.
GET 4 30209 Upper West Flamingo
ROUTE Modpul RatingFlamingoDetentionBasin.RAT  
ROUTE Modpul Flamingo.Rat 1.5 <<<<1.5 means 1.5 * storage adjustment
GET 4 30212 West Flamingo above Maryland Pkwy
COMBINE
ROUTE Modpul Flamingo.Rat 2 <<<2 means 2 cascading sub routings
GET 4 30213 Flamingo below Maryland Pkwy
COMBINE
END

Testing and notes........
Two sub basins on Flamingo Wash Las Vegas Valley <<<some title line.
GET 4 30209 Upper West Flamingo
RELEASE 100 Add 100 cfs to modpul Q rating
ROUTE Modpul RatingFlamingoDetentionBasin.RAT  
ROUTE Modpul Flamingo.Rat 1.5 <<<<1.5 means 1.5 * storage adjustment
GET 4 30212 West Flamingo above Maryland Pkwy
COMBINE
DIVERSION 1888 MyDiversionRating.Rat
ROUTE Modpul Flamingo.Rat 1.2 <<<2 means 2 cascading sub routings
GET 4 30213 Flamingo below Maryland Pkwy
COMBINE
END


GET 4 1753 Upper sub Praire
GET 4 1753 Upper sub Praire
COMBINE
ROUTE Modpul Flamingo.Rat
GET 4 1753 Upper sub Praire
COMBINE
ROUTE Modpul Flamingo.Rat
ROUTE Tatum 2.5 Upper sub Praire
GET 4 1753 Upper sub Praire
Combine
END

GET 4 30212 Upper West Flamingo
ROUTE Modpul Flamingo.Rat
GET 4 30213 Upper West Flamingo
COMBINE
END


GET 4 1753 Upper sub Praire
GET 4 1753 Upper sub Praire
COMBINE
ROUTE Modpul Flamingo.Rat
GET 4 1753 Upper sub Praire
ROUTE Modpul Flamingo.Rat
ROUTE Tatum 2.5 Upper sub Praire
GET 4 1753 Upper sub Praire
Combine
END


GET 4 1754 Lower subbasin Range Cr
COMBINE  Routed and lower runoff
END My combined Flamingo flows

ROUTE Muskingum 2 0.25
ROUTE Tatum 2
ROUTE Modpul Flamingo.Rat

Your Title Line Here is a must. 
GET 4 1753 Upper sub Praire Cr (30752 is the DatatypeSite_ID for Sub Praire Cr) 
GET 4 1753 Lower sub Praire Cr (4 indiates unit values, 3=hour, 2=day) 
COMBINE 
ROUTE Tatum 2.5   travel time in hours 
GET 4 1753 Trib sub dallas river 
COMBINE 
ROUTE Muskingum 2 0.25   lag in hours and X=.25 in who knows. 
GET 4 1753 Little sub trib 
COMBINE 
GET 4 1753 Left fork sub trib 
COMBINE 
ROUTE Modpul Flamingo.Rat    you can put comments at the end of each line 
END 

(Any notes after the END command will be ignored)



